|  |  |
| --- | --- |
|   |  floors For Tents |
|   |
| NO | ITEM | UNIT | QTY | UNIT Price | TOTAL Price in SDG |
| 1 | Excavation of pit dimention (4,4) and ‏ 0.40m depth and cart away the excavated soil including‏ cleaning the site. | job | 3 |  |  |
|  |
|  |
| 2 | provide materials(azaza) and backfilling 0.40cm from pit and compacted it well with water.,include all necessary works to get the job. according to technical specification and engineer's instruction. | job | 3 |  |  |  |
|  |
|  |
|  |
| 3 | Provide materials cast a plain concrete with slop, thickness 0.15 m mix 1:3:6 and spray with water 5 days ,and install pipe 4 insh from pvc to draining the waste water to grease trap and then to filteration system ,include all necessary works to get the job. according to technical specification and engineer's instruction. | job | 3 |  |  |  |
|  |
|  |
|  |
| Total |  |  |
| Total cost includes VAT |  |  |