Specifications of Trawa center

Metal Frame
Steel pipes 4×8 cm, thickness 1.5 mm.
Columns installed every 1.2 m.
Fully welded to the wall and concrete base.
Coated with primer and paint for rust protection.
[bookmark: _GoBack]Uniform welding with finishing .
Galvanized Zinc Sheets
Thickness 0.5 mm, rust-resistant.
Covers the kitchen, with sloped roof (canopy).
Installed with a slope of 3–5% for rainwater drainage.
Fixed to the frame using adhesive tape and silicone to prevent heat and water leakage.
Installation according to specifications and under engineer supervision.
EPX Thermal Insulation
Thickness 3 cm, resistant to heat and humidity.
Installed directly beneath the zinc sheets.
Fixed with special adhesive tape to ensure stability and prevent heat leakage.
Installation according to specifications and under engineer supervision.
Metal Skins (Kitchen Facade)
Provides kitchen ventilation with galvanized wire mesh (SAKSPNDA).
Installed on the metal frame.
Coated with  anti-rust paint.
Installation according to specifications and under engineer supervision.
Steel Doors
Thickness 1.2 mm.
Equipped with heavy-duty hinges and a standard lock.
Includes painting and fittings.
Installation according to specifications and under engineer supervision.
Screws and Rubber Gaskets
Used for fixing metal sheets and insulation.
Properly distributed over all sections to prevent leakage.
Installation according to specifications and under engineer supervision.
Frame and Metal Pipes Painting
Primer + Paint coating.
Two layers for full rust protection before and after welding.
Installation according to specifications and under engineer supervision.
Zinc and Store Exterior Painting
waterproof acrylic paint.
Two layers to prevent corrosion and reduce heat absorption.
Installation according to specifications and under engineer supervision.
Roof Waterproofing
Bitumen or acrylic waterproofing coating.
One layer, with inspection after the first rainfall to verify sealing.
Installation according to specifications and under engineer supervision.
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