	Name of Tender:
Provision of minor rehabilitation works of 5 HFs in West Darfur
Tender Number SD-CRS-538747-CW-RFQ
 Publish date 9th of August 2026  
Deadline Submission date:
 23rd of August 2026 – 04 :00 PM
Please submit your bid to CRS Geneina or through E/mail 
tenders.sudan@crs.org  

  
	اسم العطاء:
تنفيذ أعمال إعادة تأهيل طفيفة ل 5 مرافق صحية في ولاية غرب دارفور

رقم العطاء
  SD-CRS-538747-CW-RFQ
تاريخ فتح التقديم:  9 اغسطس 2026 
 
تاريخ انتهاء التقديم 

 23 اغسطس 2026 04:00   العصر 
 
 
 الرجاء ارسال عرضكم الي مكتب الاغاثة الكاثلوكية او من خلال البريد الالكتروني 
tenders.sudan@crs.org 




 
 
	Dear Sir / Madam, 
CRS Sudan is looking for companies for Provision of minor rehabilitation works of 5 HFs in West Darfur
 
General Requirements 
1.  Must Be Registered to conduct the business and in compliance with federal governments tax regulations in Sudan.
2.     Past Eexperience with International Organizations, Non-Governmental Organizations, or large private companies will be an added advantage.  
4.   CRS retains the right to reject, cancel, negotiate, amend, split and accept any offer, without consideration of the lowest offer. 
5.     This is an invitation to vendors, and it is not a promise or obligation that CRS will contract with suppliers through the submitted offers.
6.   Relevant bid committee may request for physical samples of some items during evaluation process of bids. 
7. The work plan must be provided by the contractor with the tender package.
9.The banking information should be specific and clear.


	 سيدي / سيدتي العزيز(ة)
هيئة الإغاثة الكاثوليكية  برامج السودان تبحث عن شركات من المهتمين تنفيذ أعمال إعادة تأهيل طفيفة ل 5 مرافق صحية في ولاية غرب دارفور
متطلبات عامة:
1 . يجب أن يكون مسجلا لإجراء الأعمال التجارية مع ما يتوافق  ولوائح الضرائب الحكومية في السودان .
3 . الخبرة في تزويد المنظمات الدولية، المنظمات الغير حكومية، أو  الشركات الكبيرة الخاصة ستكون ميزة.
4 . تحتفظ هيئة الاغاثة الكاثوليكية بالحق في رفض، إلغاء، التفاوض، تعديل، تجزئة وقبول أي عرض، دون النظر الى أدنى عرض. .
5. هذه دعوة للموردين وليس وعد أو التزام من هيئة الإغاثة الكاثوليكية للتعاقد مع الموردين من خلال العروض المقدمة
6. قد تقوم لجنة الإحالة المعنية بطلب نماذج عينية لبعض المواد اثناء عملية تقييم العروض.
7.  يجب على المقاول تحضير الجدول الزمني لتنفيذ الاعمال على ان يتم تسليم المستند مع اوراق العطاء
9. يجب ان تكون معلومات وتفاصيل رقم الحساب واضحة.



 
	Payment Terms
1. Quotation should remain valid for a period of at least ninety sixty (60) days from the submission closing date. 
2. Payment shall be made in SDG via bank cheque or wire transfer within 15 working days from the date of receiving the correct invoice.
3. Payment shall be made upon verification and acceptance of services/goods according to contract    Purchase order. 

	     شروط الدفع :- 
يجب أن تظل العرض ساريًا لمدة تصل إلى ستين (60) يومًا من تاريخ إغلاق التقديم.1
2. يتم إجراء الدفع بالحنيه السوداني عبر شيك بنكي أو تحويل بنكي خلال خمسة عشر (15) يوم عمل من تاريخ استلام الفاتورة الصحيحة.
3. يتم إجراء الدفع بعد التحقق وقبول الخدمات وفقًا لشروط العقد أو أمر الشراء





	Acceptance of Payment Terms
Do you accept the above payment terms?
· Yes
· No
 
	الموافقة على شروط الدفع:
هل توافق على شروط الدفع اعلاه:
· اوافق 
· لا اوافق 

	Requested Information
The submission must include:
· Full legal address and contact details of the company.
· Name of company’s official owner and copy of his/her ID & passport (if available)
· Copy of company registration certificate 
· Copy of Tax Registration Certificate.
· Reference from previous similar business experience with reference contact information. 
· Bank account information if available.
· The vendor must read, sign & stamp the Attachment (2) related to CRS SUPPLIER CODE OF CONDUCT
	يجب تقديم ما يلي:    
 يجب ان يتضمن التقديم ما يلي :                  
· العنوان الكامل الصحيح وعنوان الاتصال للشركة
· اسم صاحب الشركة الرسمي مع  نسخة من البطاقة القومية او جواز السفر.
· صورة عن شهادة تسجيل الشركة
· صورة عن شهادة التسجيل الضريبي 
· المرجع من الخبرة في الاعمال السابقة المماثلة و معلومات الاتصال للمرجع
· تفاصيل معلومات الحساب المصرفي اذا امكن.
· يجب على المقاول قراءة و توقيع و ختم الملحق(2) و الخاص بالقواعد السلوكية التي تنتهجها هيئة الإغاثة الكاثوليكية.


 
 
	Bid Requirements: - 
Offers that do not meet the following will be automatically rejected regardless of price:
1. Offers must be received before the stated deadline. 
2. Offers must include all the information requested above. 
3.  Unit prices must be provided for all line items. Offers that only include totals will be rejected.
4. Bids that include mistakes in calculations within the Bill of Quantities will be excluded from competition. 
5. Bids must be submitted through CRS Zalingei or EL Geneina office to receive bids. 
6. Offers must be clean & clear. The vendor should sign and stamp next toagainst any handwritten corrections/amendment to the bid. if available or corrections made with whiteout.  
7. Offers must be complete from all sides, signed, dated, and stamped on all pages. 
8. The technical adviser of CRS will carry out quality control of the items and reserve the right to reject items did that do not match the above-mentioned specification.
9. The duration of delivery for all requested items must be clearly specifiedy 
	     
      معلومات ملء العطاء :- 
      سوف يتم رفض أي عطاء لا يلتزم بالشروط أدناه بغض النظر عن السعر:
1. سيتم رفض أي طلب يقدم بعد التاريخ والوقت المحدد لقبول العطاءات.
2. يجب أن تتضمن العروض جميع المعلومات المطلوبة أعلاه.
3. جميع الاسعار يجب ان تكتب لكل بند أو فقرة على حدة، ويتم رفض العطاءات التي تحتوي على الإجمالي فقط. 
4. سيتم استبعاد العطاء الذي يتضمن خطأ في حسابات جداول الكميات
5.  يجب تقديم العروض في مكتب المنظمة زالنجي  او الجنينة
6. العروض يجب أن تكون نظيفة وواضحة، يجب التوقيع والختم ان وجد في مكان أي تصحيح يدوي أو باستخدام قلم التصحيح الابيض.
7. يجب أن تكون العروض كاملة من جميع الجوانب، موقعة بتاريخ واضح ومختومة على جميع الصفحات.
8. سيقوم الجهة الفنية من قبل المنظمة لمطابقة المواصفات ويتم رفض أي دواء غير متطابق للمواصفات أعلاه.
9. يجب تحديد بشكل واضح  فترة تسليم كل الكميات المطلوبة 



 
	Delivery Instructions: 
1. The company biography should not exceed 10 pages.
  
Complete and stamped and signed offer must be delivered in sealed envelope with tender number on it 
SD-CRS-538747-CW-RFQ
Delivery to CRS Geneina or through E/mail 
tenders.sudan@crs.org 
	تعليمات التسليم: 
يجب ان لا تتجاوز السيرة الذاتية للشركة اكثر من 10 صفحات.
 
يجب تقديم العطاء الكامل والمختوم و الموقع  مع كافة الوثائق المطلوبة في  ظرف مغلق يكتب عليه رقم العطا 
  SD-CRS-538747-CW-RFQ
ويسلم الى مقر مكتب الاغاثة الكاثلوكية الجنينة او من خلال البريد الالكتروني 
tenders.sudan@crs.org 
 



Experience Reference List
قائمة مراجع الاعمال السابقة
 
	 
	Name of Organization
أسم
المنظمة
	Name of Person
أسم الشخص
	Name of Project أسم المشروع
	Project Start Date تاريخ المباشرة بالمشروع
	Project duration مدة تنفيذ المشروع
	Phone Number رقم الموبايل
	Email Address البريد الالكتروني

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 

	 
	 
	 
	 
	 
	 
	 
	 




	Company name:
أسم الشركة :
	 
 

	Legal address:
العنوان الثابت:
	 
 

	Telephone Number:
رقم الهاتف:
	 
 

	Email:
عنوان البريد الإلكتروني:
	 
 

	Representative Name
اسم الممثل:
	 
 

	Business Certificate Registration Number:
رقم تسجيل شهادة العمل:
	 

	Tax registration Number:
رقم التسجيل الضريبي:
	 

	Contract duration:
مدة العقد :
	 

	   Bank details: -

· Bank Name: ……………………………………

· Bank account name: …………………………

· Bank number ………………………………

· Branch: ………………………………………



  
	تفاصيل الحساب:- 

   إسم الينك : ----------------------------------------
 
اسم الحساب :----------------------------------------


رقم الحساب :  -------------------------------------  -  


الفرع -----------------------------------------------


	Do you have partnerships with any other companies (such as shared management / staff / office / bank account)?  Do you cooperate with any other companies in preparing offers or providing goods or services?
هل لديك شراكات مع أي من الشركات الأخرى ( مثل إدارة / الموظفين / المكتب حساب مشترك / البنك) ؟ هل تتعاون مع أي من الشركات الأخرى في إعداد العروض أو توفير السلع أو الخدمات؟
	 

	If the answer to the previous above question is yes, please provide details here including the names of partner companies.
إذا كان الجواب عن السؤال السابق نعم ، يرجى تقديم التفاصيل هنا بما في ذلك أسماء الشركات الشريكة 
	 

	Other comments:
ملاحظات اخرى: 
	 

	Experience / references for the related work of experience (Please attached any related contract, purchase order, certificate, etc.) that does not exceed 10 pages. References MUST include contact information.  
يجب ان يحتوي على عناوين الاتصال من مراجع الخبرة 
المرجع من الخبرة ( الرجاء ارفاق دليل من الاعمال السابقة ذات الصلة من عقود , اوراق شراء , ورقة اتمام عمل , اخرى )  لا تتجاوز عشرة اوراق.
	 
 
 
 
 



	Signature
التوقيع
	 

	Date
التاريخ
	 



ATTACHED (1)
Lot#1
Bill Of Quantities for Rehabilitation fence and two rooms with Waiting Area

	West  Darfur      -     Aboghabina health facility 

	N O
	Description
	Unit 
	Quantity
	Unit Price SDG
	Amount SDG

	 
	fence 

	 
	"Provide material and fabricate a gate for the fence with a total width of 3 meters, consisting of three leaves. The gate shall be constructed from iron box sections as per the engineer's instructions and fixed between brick columns and a rammed base. The entire structure shall be finished with plastering and painting
	Pcs
	1
	 
	 

	 
	Provide material and fix  in position Metal Boundary Fence composed of vertical posts Cylindrical 3 inch diameter, 1mm thickness, and  2.5 m length, Penetrate 50 cm and fix by concrete base 40 cm X 40 cm X 60 cm each 2 m C/C and 45 degree slope support of  2.5 X 2.5 inch  angle @ 6 m C/C and corners ,the horizontal elements tension wires 4 rows to fix chain-link mesh 50 mm X 50 mm (Gabyan ) to the  Satisfaction  of the engineer ,sample to be approved in advance
	Meter Length (ML)
	          135.0 
	 
	 

	 
	sub total
	 
	 
	 
	                                          -   

	 
	  Two rooms and attached waiting Area 

	7
	provide material construct and lay plaster (1:8 cement sand mortar) internal and external include (barabied) and crossings of windows and doors
	M²
	          200.0 
	 
	 

	9
	Provide material and back fill using selected material in side the building up to depth 50 cm above Zero level in 3 layers
	M3
	               8.0 
	 
	 

	10
	provide material  and casting plain concrete with depth 10 cm use mix 1:3:6 fair face finish
	M3
	             39.0 
	 
	 

	 
	provide and install taile 
	M²
	             39.0 
	 
	 

	 
	provide material  and install skirt 
	ML
	             43.0 
	 
	 

	11
	provide and apply painting in walls, internally and external wall  should be smooth surface finish use gypsum/filler or silky and apply plastic emulsion (Bomastic) in 3 coats , 
	M²
	          200.0 
	 
	 

	12
	 provide material and fix steel door  size 1 mx2.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	No.
	               2.0 
	 
	 

	13
	 provide and fix steel window with fine mesh and sixbanda  size 1 mx1.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	No.
	               5.0 
	 
	 

	 
	sub total 
	 
	 
	 
	 

	 
	Construct new block  latrine with three drop holes  and water storage

	1
	Excavate hole for a 2 block communal latrine size 2.6 mX 4. 5 m  and 4 m depth.
	M3
	47
	 
	 

	2
	provide material and construct and build  brick wall around hole for lining by using thickness one brick and half(first class burn brick size 11cm x6cm x22 cm) must rise 0.5 m from zero level,use cement /sand mortar 
	M²
	64
	 
	 

	3
	provide material and casting plain concrete with depth 10 cm use mix 1:3:6 
	M²
	12
	 
	 

	4
	provide  material and cast reinforced concrete (1:2:4) mix for tie beam with section 30 cmx 30 cm  use steel bar 12 mm 4T12@150mmc/c  As shown in drawing
	ML
	14
	 
	 

	5
	construct and cast reinforce concrete slabs use mix (1:2:4)  thickness of 15 cm using 12 mm steel  bar with 150 mm spacing (Y12@15 cm c/c) with  manholesize 30cm x 30 cm
	M²
	12
	 
	 

	6
	provide material construct and build brick wall for  three rooms communal latrine , and
Privacy  wall by using thickness one brick (first class burn brick size 11cm x6cm x22 cm)     ,use cement morter including Barbate. 
	M²
	35
	 
	 

	7
	Provide  material and cast reinforce concrete lentel Beam use mix (1:2:4)  thickness of 10 cm using 10 mm steel  bar with strips 150 mm spacing (6mm@15 cm c/c)
	ML
	4.5
	 
	 

	8
	Excavate strip foundation with width 40 cm and depth 45 cm  for privacy wall
	ML
	13.5
	 
	 

	9
	provide  material  and construct   cut off wall using thickness one and half brick (first class burned brick size 11cm x6cm x22 cm) with height 30 cm  above Zero level, use cement/sand mix 1:9
	ML
	13.5
	 
	 

	10
	Provide  material and back fill using selected material in side the building up to dept 50 cm above Zero level in 3 layers
	M³
	7
	 
	 

	11
	provide material construct and build  brick wall with height 1.8 m by using thickness one brick  (first class burn brick size 11cm x6cm x22 cm ,use cement /sand mortar 
	M²
	24
	 
	 

	12
	Provide material  and install heavy metal doors (180 cm X 0.8cm)  framed with hollow steel pipe and it has sky light with hight 20cm at top use mesh (fine and sixbanda)
	Pcs
	3
	 
	 

	13
	 provide material fixing squat seats  for latrine 
	Pcs
	3
	 
	 

	 
	provide  material and install taile 
	M²
	18.5
	 
	 

	 
	provide and install skirt
	ML
	28
	 
	 

	14
	Provide  material  and fix ventilation  PVC pipe 3 inchs (3 meters Apove slab) covered with mesh at top
	No.
	2
	 
	 

	15
	provide material and construct and lay plaster ( 1:8  cement sand mortar) internal and external include (barabied)
	M²
	118
	 
	 

	16
	provide  material and fix sky light framed from steel Angle and mesh (fine and sixbanda) size 35 cm x 35 cm
	No.
	3
	 
	 

	17
	provide and apply painting in walls, internally and external wall  should be smooth surface finish use gypsum/filler or silky and apply plastic emulsion (Bomastic) in 3 coats ,  
	M²
	118
	 
	 

	18
	provide material and construct and install iron corrugated sheets (zinc 35) for roof complete with steel rafters (use steel hollow pipes 3cm x 6 cm ) 
	M²
	8
	 
	 

	19
	provide material and construct and cast plain concrete with depth 10 cm
	M²
	13.5
	 
	 

	20
	Provide  material and install public water basin wash with one taps including all necessary water connection fitting and connected with water tank 
	No.
	2
	 
	 

	21
	Provide  material and fix ( biba) 
	No.
	2
	 
	 

	22
	provide  material and build Giltrab size 30x30 cm with reinforced concrete cover 
	No.
	2
	 
	 

	23
	Provide  material and build mainhole size 50x50 cm with  reinforced  concrete cover with connected to  Giltrab and pit using P V C Pipe 4 inch
	No.
	2
	 
	 

	24
	Excavite pit with section 2 mx2m and depth 3m and back fill with crashed brick include 4 layers of charcool jn 10cm  
	job
	1
	 
	 

	25
	provide material and costruct base for water storge 1500 litter using red bricks and sand / cement morter in size 2.5 m x 2.5 m and height 1.5 m and cover at top by reinforced concrate thickness 12 cm and costruct steps leader  with hand rails as instructed by engineer
	job
	1
	 
	 

	26
	Provide and install a 1,500‑liter horizontal Tiga water storage tank, and extend two tap lines — one to the latrine and one for health facility consumption — with a total pipeline length of 25 m.
	job
	1
	 
	 

	
	Sub Total
	 
	 
	 
	                            -   

	 
	Constructing new wainting area shelter for OTP benefiecary

	1
	Excavate strip foundation with width 60 cm and depth 60 cm and back fill with stone up to level 40 cm 
	Meter Length(ML)
	25.5
	 
	 

	2
	Excavate strip foundation with width 50 cm and depth 50 cm and back fill with stone up to level 30 cm for attached  waiting Area shelter
	Meter Length(ML)
	29
	 
	 

	3
	provide and construct   brick wall using thickness two brick (first class burn brick size 11cm x6cm x22 cm) with hight 20 cm above Zero level,use cement/sand mix 1:8
	Meter Length(ML)
	25.5
	 
	 

	4
	provide and construct   brick wall using thickness one and half brick (first class burn brick size 11cm x6cm x22 cm) with hight 30 cm above Zero level,use cement/sand mix 1:8 for attached  waiting Area shelter 
	Meter Length(ML)
	29
	 
	 

	5
	provide andconstruct and cast reinforced concrete (1:2:4) mix for grade beam with section 30 cmx 30 cm  use steel bar 12 mm 5T12@150mmc/c  As shown in drawing
	Meter Length(ML)
	25.5
	 
	 

	6
	provide and construct and cast reinforced concrete (1:2:4) mix for lentil beam with section 35 cmx 15 cm  use steel bar 12 mm 5T12@150mmc/c  As shown in drawing
	Meter Length(ML)
	25.5
	 
	 

	7
	provide and construct and build  brick wall including Barbate   by using thickness one and half brick (first class burn brick size 11cm x6cm x22 cm) ,use mud morter
	Square meter( M²)
	102
	 
	 

	8
	Provide and costruct brick wall 25 cm thickness with suports each 2 m using cement /sand morter Mix   ( 1: 6 ) for waiting Area shelter
	Square meter( M²)
	35
	 
	 

	9
	provide and back filling using selected soil with well compacted in 3 layers for both room and attached waiting Area shelter
	Cubic meter (M³)
	26
	 
	 

	10
	Provide and casting plain concrete with 10 cm thickness with curing using water for 7 days for both room and attached waiting Area shelter
	Square meter( M²)
	72
	 
	 

	11
	provide and fix roof using UK zinc sheet(0.35mm) and Iron pipe 4 cm X 8 cm , 1mm  thickness              as shown in drawing for both room and attached waiting Area shelter
	Square meter( M²)
	80
	 
	 

	12
	provide and install zinc sheet on upper side of shelter Hanging 100 cm using (American sheets )
	Meter Length(ML)
	29
	 
	 

	13
	provide and fix Cylindrical iron pipe 3 inch in diameter , 3.5 m length and 1mm thickness for shelter witt painting
	Pcs
	14
	 
	 

	14
	Provide and plastering wall using cement/sand mortar mix 1:8 or both room and attached waiting Area shelter
	Square meter( M²)
	274
	 
	 

	15
	provide and apply painting in walls, internally and external wall  should be smooth surface finish use gypsum/filler or silky and apply plastic emulsion (Bomastic) in 3 coats , 
	Square meter( M²)
	274
	 
	 

	16
	Provide and fix  mesh (sixbenda) wit section 2 m length and 1 m height on shelter side 
	Pcs
	15
	 
	 

	17
	Provide and fix Doors with section 2 m X  1 m for shelter
	Pcs
	1
	 
	 

	18
	 provide and fix steel door  size 1 mx2.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	Pcs
	2
	 
	 

	19
	 provide and fix steel window with fine mesh and sixbanda  size 1 mx1.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	Pcs
	3
	 
	 

	20
	 provide and fix sky light with fine mesh and sixbanda  size 40 cm x 40 cm 
	 
	2
	 
	 

	 
	Sub total 
	 
	 
	 
	 



Lot#2

	West Darfur      -     Karrak  health facility 

	Bill Of Quantities for Rehabilitation fence and four rooms, latrine and water storge 

	N O
	Description
	Unit 
	Quantity
	Unit Price SDG
	Amount SDG

	A
	fence 

	1
	"Provide material and fabricate a gate for the fence with a total width of 3 meters, consisting of three leaves. The gate shall be constructed from iron box sections as per the engineer's instructions, and fixed between brick columns and a rammed base. The entire structure shall be finished with plastering and painting
	Pcs
	               1.0 
	 
	 

	2
	Provide material  and fix  in position Metal Boundary Fence composed of vertical posts Cylindrical 3 inch diameter 2.5 m length, Penetrate 50 cm and fix by concrete base 40 cm X 40 cm X 60 cm each 2 m C/C and 45 degree slope support of  2.5 X 2.5 inch  angle @ 6 m C/C and corners ,the horizontal elements tension wires 4 rows to fix chain-link mesh 50 mm X 50 mm (Gabyan ) to the  Satisfaction  of the engineer ,sample to be approved in advance
	Meter Length (ML)
	          135.0 
	 
	 

	 
	Total sub budget  1
	 
	 
	 
	 

	1
	  four roms ,water storge and latrine

	2
	provide and install taile 
	M²
	             82.0 
	 
	 

	3
	provide material  and install skirt 
	ML
	             93.0 
	 
	 

	4
	provide and apply painting in walls, internally and external wall  should be smooth surface finish use gypsum/filler or silky and apply plastic emulsion (Bomastic) in 3 coats , 
	M²
	          200.0 
	 
	 

	5
	 provide material and do  minor repairefor and painting  for steel door  size 1 mx2.2 
	No.
	               4.0 
	 
	 

	6
	 provide and  do  minor repairefor and painting for  steel window with fine mesh and sixbanda  size 1 m x 1.2 m
	No.
	               7.0 
	 
	 

	7
	 provide material and do  minor repairefor and painting  for steel door  size 80 cm x  200 cm
	No.
	               4.0 
	 
	 

	8
	provide material and cast lentil beam for latrine cross section 25 cm x 10 cm 
	ML
	               5.5 
	 
	 

	9
	excavate strip foundation for privacy wall 40 cm x 40 cm 
	ML
	             14.0 
	 
	 

	10
	provide material and construct cut off wall using thickness one and half  brick (first class burn brick size 11cm x6cm x22 cm)     ,sand cement  morter
	ML
	             14.0 
	 
	 

	11
	provide material construct and build brick wall to rise 60 cm for   four rooms communal latrine  , and
Privacy  wall with heightb180 cm by using thickness one brick (first class burn brick size 11cm x6cm x22 cm)     ,use cement morter including Barbate. 
	M²
	             39.0 
	 
	 

	12
	provide material and cast plain concrete depth 10 cm for latrine privacy yard using mix 1:3:6
	M²
	             12.0 
	 
	 

	13
	provide material and construct and install iron corrugated sheets (zinc 35) for roof complete with steel rafters (use steel hollow pipes 3cm x 6 cm ) 
	M²
	               8.1 
	 
	 

	14
	provide material and install squat seat for latrine 
	N.o
	               4.0 
	 
	 

	15
	Provide  material and install public water basin wash with one taps including all necessary water connection fitting and connected with water tank 
	N.o
	               2.0 
	 
	 

	16
	provide material and costruct base for water storge 1500 litter using red bricks and sand / cement morter in size 2.5 m x 2.5 m and height 1.5 m and cover at top by reinforced concrate thickness 12 cm and costruct steps leader  with hand rails as instructed by engineer
	Job
	               1.0 
	 
	 

	17
	provide water storge 1500 liters  horizantal ( tiga ) and extend 2 tapsline one to latrine and second for HF use
	Job
	               1.0 
	 
	 

	18
	Total sub budget  2
	 
	 
	 
	 

	 
	Constructing new waiting area shelter for OTP beneficiary

	1
	Excavate strip foundation with width 60 cm and depth 60 cm and back fill with stone up to level 40 cm 
	Meter Length(ML)
	25.5
	 
	 

	2
	Excavate strip foundation with width 50 cm and depth 50 cm and back fill with stone up to level 30 cm for attached  waiting Area shelter
	Meter Length(ML)
	29
	 
	 

	3
	provide and construct   brick wall using thickness two brick (first class burn brick size 11cm x6cm x22 cm) with hight 20 cm above Zero level,use cement/sand mix 1:8
	Meter Length(ML)
	25.5
	 
	 

	4
	provide and construct   brick wall using thickness one and half brick (first class burn brick size 11cm x6cm x22 cm) with hight 30 cm above Zero level,use cement/sand mix 1:8 for attached  waiting Area shelter 
	Meter Length(ML)
	29
	 
	 

	5
	provide andconstruct and cast reinforced concrete (1:2:4) mix for grade beam with section 30 cmx 30 cm  use steel bar 12 mm 5T12@150mmc/c  As shown in drawing
	Meter Length(ML)
	25.5
	 
	 

	6
	provide and construct and cast reinforced concrete (1:2:4) mix for lentil beam with section 35 cmx 15 cm  use steel bar 12 mm 5T12@150mmc/c  As shown in drawing
	Meter Length(ML)
	25.5
	 
	 

	7
	provide and construct and build  brick wall including Barbate   by using thickness one and half brick (first class burn brick size 11cm x6cm x22 cm) ,use mud morter
	Square meter( M²)
	102
	 
	 

	8
	Provide and costruct brick wall 25 cm thickness with suports each 2 m using cement /sand morter Mix   ( 1: 6 ) for waiting Area shelter
	Square meter( M²)
	35
	 
	 

	9
	provide and back filling using selected soil with well compacted in 3 layers for both room and attached waiting Area shelter
	Cubic meter (M³)
	26
	 
	 

	10
	Provide and casting plain concrete with 10 cm thickness with curing using water for 7 days for both room and attached waiting Area shelter
	Square meter( M²)
	72
	 
	 

	11
	provide and fix roof using UK zinc sheet(0.35mm) and Iron pipe 4 cm X 8 cm , 1mm  thickness              as shown in drawing for both room and attached waiting Area shelter
	Square meter( M²)
	80
	 
	 

	12
	provide and install zinc sheet on upper side of shelter Hanging 100 cm using (American sheets )
	Meter Length(ML)
	29
	 
	 

	13
	provide and fix Cylindrical iron pipe 3 inch in diameter , 3.5 m length and 1mm thickness for shelter witt painting
	Pcs
	14
	 
	 

	14
	Provide and plastering wall using cement/sand mortar mix 1:8 or both room and attached waiting Area shelter
	Square meter( M²)
	274
	 
	 

	15
	provide and apply painting in walls, internally and external wall  should be smooth surface finish use gypsum/filler or silky and apply plastic emulsion (Bomastic) in 3 coats , 
	Square meter( M²)
	274
	 
	 

	16
	Provide and fix  mesh (sixbenda) wit section 2 m length and 1 m height on shelter side 
	Pcs
	15
	 
	 

	17
	Provide and fix Doors with section 2 m X  1 m for shelter
	Pcs
	1
	 
	 

	18
	 provide and fix steel door  size 1 mx2.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	Pcs
	2
	 
	 

	19
	 provide and fix steel window with fine mesh and sixbanda  size 1 mx1.2 m(accomy) with 20 cm opening in upper side covered by fiber using screw 
	Pcs
	3
	 
	 

	20
	 provide and fix sky light with fine mesh and sixbanda  size 40 cm x 40 cm 
	 
	2
	 
	 

	 
	Total sub budget 3
	 
	 
	 
	 

	 
	Total budget 1+2+3
	 
	 
	 
	 



Lot#3

	West Darfur      -     Tandality   health facility 

	Bill Of Quantities for Rehabilitation fence, water store , ten rooms and latrine 

	N O
	Description
	Unit 
	Quantity
	Unit Price SDG
	Amount SDG

	1
	  ten roms ,water storge and latrine

	2
	provide and install taile for RH rooms ,conslutation ,dressing , EPI and latrine
	M²
	          158.0 
	 
	 

	3
	provide material  and install skirt for RH rooms ,conslutation ,dressing , EPI and latrine
	ML
	          140.0 
	 
	 

	4
	Provide all necessary materials, labor, tools, and equipment to carry out the rehabilitation of major cracks in brick walls across the Delivery Room.
Scope of work shall include:
Cleaning and preparation of cracked areas.
Stitching, filling, and sealing of cracks using appropriate mortar or repair compounds.
Repointing and finishing to match existing wall surfaces.
Ensuring structural integrity and aesthetic consistency after repair.
	Job
	               1.0 
	 
	 

	5
	Provide all necessary materials, labor, tools, and equipment to:
Close the existing door opening on the north side, dimensions 2.2 m × 1.0 m.Create a new door opening on the west side, dimensions 2.2 m × 1.0 m, between rooms.
Reinstall the previously removed door unit in the new opening.
	Job
	               1.0 
	 
	 

	6
	provide and apply painting in walls, internally and external wall  should be smooth surface finish use gypsum/filler or silky and apply plastic emulsion (Bomastic) in 3 coats , 
	M²
	       1,018.0 
	 
	 

	7
	 provide material and do  minor repairefor and painting  for steel door  size 1 mx2.2 
	No.
	             11.0 
	 
	 

	8
	 provide and  do  minor repairefor and painting for  steel window with fine mesh and sixbanda  size 1 m x 1.2 m
	No.
	             22.0 
	 
	 

	9
	 provide material and do  minor repairefor and painting  for steel door  size 80 cm x  200 cm
	No.
	               2.0 
	 
	 

	10
	provide material and install squat seat for latrine 
	N.o
	               2.0 
	 
	 

	11
	Provide  material and install public water basin wash with one taps including all necessary water connection fitting and connected with water tank 
	N.o
	               1.0 
	 
	 

	12
	provide material and costruct base for water storge 1500 litter using red bricks and sand / cement morter in size 2.5 m x 2.5 m and height 1.5 m and cover at top by reinforced concrate thickness 12 cm and costruct steps leader  with hand rails as instructed by engineer
	Job
	               1.0 
	 
	 

	13
	provide water storge 1500 liters  horizantal ( tiga ) and extend 2 tapsline one to latrine and second for HF use
	Job
	               1.0 
	 
	 

	 
	Total  
	 
	 
	 
	 



Lot#4

	West Darfur      -     Korgei   health facility 

	BoQ for renovation in Korgei Healyh Facility 

	N O
	Description of Items
	Unit 
	Quantity
	unit price SDG
	Amount SDG

	 
	Rehabilitation of Major Cracks in Brick Walls Using Tie Beams
	 
	 
	 
	 

	1
	provide all necessary materials, labor, tools, and equipment to carry out the rehabilitation of major cracks in brick walls across the following rooms: Nutrition section, Dressing Room, Delivery Room, Waiting Area, and Consultation Room.•note  : Ensure proper finishing and curing of all concrete works
	 
	 
	 
	 

	1.1
	• Install two reinforced concrete tie beams along the crack line in each of the following rooms:
• Nutrition Room, Dressing Room, and Delivery Room: Tie beams with dimensions 25 cm x 10 cm x 1 m.
• Waiting Area and Consultation Room: Tie beams with dimensions 25 cm x 10 cm x 2.5 m.
• Carefully remove the affected portions of the wall and roof to access the cracked areas.
• Install steel reinforcement and cast the tie beams using appropriate concrete grade.
• Reconstruct the demolished wall and roof sections after tie beam installation.
	Job
	1
	 
	 

	2
	floor
	 
	 
	 
	 

	2.1
	Removal and Replacement of Damaged Floor Sections with Compacted Sand
	 
	 
	 
	 

	 
	Provide material cast plan concrete Mix 1:3:6 and  for damaged area at waiting area and some rooms
	M²
	25
	 
	 

	2.2
	provide materials  and lay ceramic taile for dressing  , consultion ,drug store,EPI and reproductive unit 
	M²
	133
	 
	 

	2.3
	provide materials  and install skirt (Wazar)
	ML
	113
	 
	 

	3
	Roof
	 
	 
	 
	 

	3.1
	Provide all necessary materials, labor, tools, and equipment to carry out roof repair and maintenance works for the Reproductive Unit,  Dressing Room, Consultation Room, Drug Store, EPI, and OTP sections.
Scope of work shall include:
Cleaning and preparation of roof surfaces.
Use of suitable methods and materials to maintain and repair damaged zinc sheets.
Ensuring proper waterproofing to prevent water leakage.
All works to be executed as identified and approved by the Engineer.
	job 
	1
	 
	 

	4
	 painting 
	 
	 
	 
	 

	4.1
	Provide all necessary materials, labor, tools, and equipment to carry out painting works on internal walls of the  Reproductive Unit,  Dressing Room, Consultation Room, Drug Store, EPI, and OTP sections.
Scope of work shall include:
Cleaning and preparation of wall surfaces.Application of three coats of emulsion paint (Bomastic).
Final color selection to be identified and approved by the Enginee
	M²
	730
	 
	 

	5
	Doors and windows 
	 
	 
	 
	 

	5.1
	Provide all necessary materials, labor, tools, and equipment to supply and install a door leaf with lock, fixed to the existing wall frame (already in place), including:
Proper fitting and alignment of the door leaf (size 1.0 m × 2.20 m).
Installation of lockset and associated hardware.
Surface preparation and painting of the door as per specifications.
Final finish and color to be approved by the Engineer.
	No.
	8
	 
	 

	5.2
	Provide all necessary materials, labor, tools, and equipment to supply and install awindow leaf  fixed to the existing wall frame (already in place), including:
Proper fitting and alignment of the door leaf (size 1.0 m × 1 m).
Installation of  fiber at upper side of frame.
Surface preparation and painting of the window as per specifications.
Final finish and color to be approved by the Engineer.
	No.
	14
	 
	 

	6
	water supply 
	 
	 
	 
	 

	6.1
	provide material and costruct base for water storge 1500 litter using red bricks and sand / cement morter in size 2.5 m x 2.5 m and height 1.5 m and cover at top by reinforced concrate thickness 12 cm and costruct steps leader  with hand rails as instructed by engineer
	Job
	1
	 
	 

	6.2
	provide water storge 1500 liters  horizantal ( tiga ) and extend 2 tapsline one to latrine and second for HF use
	Job
	1
	 
	 

	6
	Total
	 
	 
	 
	 








Lot#5
	West  Darfur      -     Tanjakei  health facility 

	Bill Of Quantities for Rehabilitation fence , water storge , seven  rooms , waiting area and nutrition center 

	N O
	Description
	Unit
	Quantity
	Unit Price SDG
	Amount SDG

	1
	  Eight rooms, waiting area , nutrition center  

	2
	provide material and install taile for nutrition center  ,consultation , drug store ,dressing ,  short stay ,EPI and waiting area
	M²
	          163.0 
	 
	 

	3
	provide material and install skirt for  waiting area  ,conslutation ,dressing , EPI 
	ML
	          105.0 
	 
	 

	4
	Provide all necessary materials, labor, tools, and equipment to carry out the rehabilitation of major cracks in brick walls across the, conslutation ,dressing , EPI and drug store and nutrition section
Scope of work shall include:
Cleaning and preparation of cracked areas.
Stitching, filling, and sealing of cracks using appropriate mortar or repair compounds.
Repointing and finishing to match existing wall surfaces.
Ensuring structural integrity and aesthetic consistency after repair.
	Job
	               1.0 
	 
	 

	 
	excavate strip foundation with cross section 30 cm x 30 cm
	ML
	               4.0 
	 
	 

	 
	Provide and construct a 1½‑brick thick first‑class burnt brick wall (brick size 11 cm × 6 cm × 22 cm), plastered with cement–sand mix 1:8, up to 3 m height above zero level inside the nutrition center, to partition a store of 2.4 m × 4.3 m with a door opening of 2.2 m × 1 m, and to close the skylight opening at the upper wall.
	M²
	             16.0 
	 
	 

	 
	provide material and steel door ( Ecommay) size 2.2 m x 1 m for smll nutrition store 
	No.
	               1.0 
	 
	 

	 
	provide material and fix roof using UK zinc sheet(0.35mm) and Iron pipe 4 cm X 8 cm , 1mm  thickness  at nitrition center 
	M²
	             14.0 
	 
	 

	 
	Provide and fix  mesh (sixbenda) wit section 2 m length and 0.5 m height on nutrition center 
	No.
	               8.0 
	 
	 

	6
	provide and apply painting in walls, internally and external wall  should be smooth surface finish use gypsum/filler or silky and apply plastic emulsion (Bomastic) in 3 coats , 
	M²
	          975.0 
	 
	 

	7
	"Provide all necessary materials, labor, and equipment to carry out repair, minor  maintenance, and painting works for steel door, size 1.0 m × 2.2 m
	No.
	               8.0 
	 
	 

	8
	"Provide all necessary materials, labor, and equipment to carry out repair,minor  maintenance, and painting works for  steel window , size 1.0 m × 2.2 m
	No.
	             18.0 
	 
	 

	14
	Sub total 
	 
	 
	 
	 

	 
	Total  A + B
	 
	 
	 
	 




ATTACHED (2)
Scope of Work (SoW) for Rehabilitation of Health Center Facilities in El Geneina, Serba, and Kereinek Localities, West Darfur
Catholic Relief Services (CRS) intends to rehabilitate selected health center facilities located in El Geneina, Serba, and Kereinek Localities, West Darfur State, Sudan. The rehabilitation works aim to restore and improve the functionality, safety, and quality of healthcare infrastructure to ensure the delivery of essential health services in accordance with Ministry of Health standards and humanitarian best practices. CRS infrastructure projects typically prioritize safety, functional facilities with reliable water, sanitation, and quality construction.
The contractor shall provide all labor, materials, equipment, tools, transportation, supervision, and technical services necessary to complete the rehabilitation works.
The contractor’s responsibilities:
The specific tasks of the contractor under this scope of work should be implemented under direct supervision and instruction of CRS field staff, and each completed stage of the work should be accepted and approved by CRS field staff, and the contractor should implement and complete any required repair or amendment before starting the next stage, also contractor should be responsible to the following:
1- Materials
· All materials shall be new, unused, and approved quality by Project Engineer
· The materials shall be complied with the technical specifications and applicable Sudanese or internationally recognized standards
· Samples shall be submitted for approval by Project Engineer before procurement where required.


2- Quality Control
The contractor shall:
· Implement a quality control system throughout the rehabilitation period.
· Conduct all required inspections and testing (if need).
· Correct defective work at no additional cost
· Maintain records of inspections and test results.
3- Health, Safety, and Environmental (HSE) Requirements
The contractor shall
· Comply with national occupational health and safety regulations and CRS safety requirements.
· Provide appropriate personal protective equipment (PPE) to all workers
· Maintain first did facilities on site.
· Prevent environmental pollution.
· Control dust, noise, and rehabilitation waste.
· Protect patients, health workers, and visitors during rehabilitation activities.
4- Environmental and Social Safeguards
The contractor shall:
· Minimize disruption to health services.
· Ensure safe access for patients and staff.
· Prevent child labor and forced labor.
· Prevent gender-based violence, sexual exploitation, abuse, and harassment (GBV/SEAH).
· Respect local communities and cultural practices.
· Adhere to CRS safeguarding and code of conduct requirement.
5- Schedule
· Commence works immediately upon receipt of the notice proceed.
· Complete all work within the period specified in the contract.
· Submit a detailed work program showing activity sequencing, milestones and completion dates.
       6- Inspection and Supervision
        The works shall be supervised by CRS and/or designated Engineer. The contractor shall:
· Provide unrestricted access to the site.
· Cooperate during inspections.
· Rectify defects identified during inspections within the specified timeframe.
        7- Testing and Commissioning
           The contractor shall perform all required testing and commissioning of electrical,     
       plumbing, and other building systems before handing over.
         8- Handover
             Upon completion, the contractor shall:
· Thoroughly clean the site 
· Remove temporary work and unused materials
· Submit as-built drawings where applicable.
· Provide warranties and operation manual for installed equipment.
· Remedy all defects identified during the Defect Liability period.
         9- Deliverables 
             The contractor shall submit:
· Work program and implementation schedule.
· Materials submittals and approvals.
· Quality assurance documentation.
· Weekly or biweekly progress reports.
· Inspection and testing records.
· Completion report.
· As-built drawings (where applicable).
· Defect liability commitments.




         10- Applicable Documents
             The work shall be executed in accordance with:
· Approval architectural, structural, electrical, and plumbing drawings.
· Technical Specifications.
· Bill of Quantities (BoQ).
· Contract Conditions.
· CRS construction standards and safeguarding requirements.
· Applicable Sudanese Building codes and Ministry of Health requirements.



        
	
Bidder’s (Company) Name: ________________

Authorized Person Full Name: _____________
Title (Position):	_________________________

Signature and Company Official Stamp:	_____

Date: ____________________

	
اسم مقدم العرض (الشركة)___________________

الاسم الكامل للشخص المفوض: _________________ 

اللقب (المنصب): ___________________________

التوقيع وختم الشركة الرسمي: _______________

التاريخ:___________________________




      



