|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | soak pit for kitchen | | | | |
|  | | | | | |
| NO | ITEM | UNIT | QTY | UNIT Price | TOTAL Price in SDG |
| 1 | Excavation of pit dimention (1.2,1.2) and 2m depth and cart away the excavated soil including‏ cleaning the site. | m3 | 2 |  |  |
|  |
|  |
| 2 | provide materials and build a wall around the pit | m3 | 9.6 |  |  |  |
|  |
|  |
|  |
| 3 | Provide materials (damaged brik & sand) cast it into the pit. | job | 1 |  |  |  |
|  |
|  |
| 4 | provide materials and install cover for pit from iron sheet and rectangle pipe | number | 1 |  |  |  |
| total | | | | |  |  |
| Total Cost with Vat | | | | |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | soak pit for showers (2\*2\*2) | | | | |
|  | | | | | |
| NO | ITEM | UNIT | QTY | UNIT Price | TOTAL Price in SDG |
| 1 | Excavation of pit dimention (2,2) and 2m depth and cart away the excavated soil including‏ cleaning the site. | m3 | 8 |  |  |
|  |
|  |
| 2 | provide materials and build a wall around the pit ,include all necessary works to get the job. according to technical specification and engineer's instruction. | m3 | 16 |  |  |  |
|  |
|  |
|  |
| 3 | Provide materials (damaged brik & sand) cast it into the pit.,include all necessary works to get the job. according to technical specification and engineer's instruction. | jop | 1 |  |  |  |
|  |
|  |
|  |
| 4 | providd materials and install cover for pit from iron sheet and rectangle pipe. | number | 1 |  |  |  |
| total | | | | |  |  |
| Total Cost with Vat | | | | |  |  |
|  | | | | | |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | fences | | | | |
|  | | | | | |
| NO | ITEM | UNIT | QTY | UNIT Price | TOTAL Price in SDG |
| 1 | provide materials and build partition high 2m long 30 from iron sheet (زنك ليبي)and angle 2.5 in ,5mm and do supportive after each 4 meters ,include all necessary works to get the job. according to technical specification and engineer's instruction. | jop | 1 |  |  |
|  |
|  |
| 2 | provide materials and build partition to waste area high 2m to the area 10\*4 from iron sheet (زنك ليبي)and angle 2.5 in ,5mm ,include all necessary works to get the job. according to technical specification and engineer's instruction. | jop | 1 |  |  |  |
|  |
|  |
|  |
| total | | | | |  |  |
| Total Cost with Vat | | | | |  |  |