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Amendment No. 1
This Amendment forms an integral part of the Bidding Document. The provisions identified below are amended accordingly. Except as expressly amended herein, all other provisions of the Bidding Document remain unchanged.
	Item No. 1
	Perimeter Security Fence Quantity
In Section VII – Works’ Requirements, Annex 2: Bill of Quantities, BoQ 1 – BoQ for Solarization of School, Item 1.3.2, the quantity for the perimeter security fence is amended as follows:
Existing quantity:
50 meters
Amended quantity:
60 linear meters per school
Accordingly, bidders shall price 60 linear meters under BoQ Item 1.3.2 for each school.

	Item No. 2
	Fence Post Foundation Dimensions
In Section VII – Works’ Requirements, Drawing Sheet A.01.06 – Solar Panel Typical Module Design – Fence Design, the fence post foundation dimensions are amended as follows:
Existing dimensions:
50 cm × 50 cm × 100 cm
Amended dimensions:
40 cm × 40 cm × 60 cm
The amended dimensions are consistent with BoQ Item 1.3.2. The amended drawing attached to this Amendment replaces the corresponding provision in the originally issued drawing.

	Item No. 3
	Structural Steel Purlin Dimensions
In Section VII – Works’ Requirements, Drawing Sheet A.01.05 – Solar Panel Typical Module Design – Side and Front View, the following notations are amended:
Existing notation:
“4 × 8 mm, 1 mm thick Steel Pipe”
Amended notation:
“40 mm × 80 mm rectangular steel pipe, 1 mm thick”
Existing notation:
“3 × 6 mm, 1 mm thick Steel Pipe”
Amended notation:
“30 mm × 60 mm rectangular steel pipe, 1 mm thick”
The amended drawing attached to this Amendment replaces the corresponding provision in the originally issued drawing.

	Item No. 4
	Project Manager Qualification
In Section VII – Works’ Requirements, Key Personnel table, the academic qualification specified for the Project Manager is amended as follows:
Existing requirement:
Bachelor’s Degree in Civil Engineering
Amended requirement:
Bachelor’s Degree in Electrical Engineering
The requirement for at least five years of relevant experience in solar projects remains unchanged.

	Item No. 5
	Pricing of Signboards
In Section VII – Works’ Requirements, Key Activities, Subsection 1: Preliminaries, Safety and Site Management (BoQ 0), the pricing of signboards is clarified as follows:
For avoidance of doubt, BoQ 0, Item 1.2 relates to temporary electrical and water supply and associated running costs and does not include signboards. Bidders shall price the required signboards exclusively under the dedicated signboard line item in the respective Lot Financial Offer table. No additional signboard cost shall be included in the BoQ 0 lump-sum items.
The applicable quantities are:
· Lot 1 – Al Rahad: 5 signboards 
· Lot 2 – Al Fashaga: 1 signboard 
· Lot 3 – Al Fao: 3 signboards 
· Lot 4 – Basundah: 6 signboards


Attachment
Revised Drawing Set
The attached Revised Drawing Set replaces the drawing set originally issued with the Bidding Document solely to incorporate the amendments specified under Items No. 2 and 3 above. All other requirements of the Bidding Document remain unchanged.
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