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Clarification to Queries No. 1
	Question No. 1
	Perimeter Security Fence Dimensions and BoQ Quantity
BoQ Item 1.3.2 specifies fence dimensions of 15 m × 15 m, which corresponds to a total perimeter of 60 linear meters. However, the quantity indicated in the BoQ is 50 meters per school. Please confirm whether bidders should price 50 linear meters or 60 linear meters for a complete 15 m × 15 m enclosure.

	Response
	The required quantity is 60 linear meters per school. Accordingly, bidders shall price 60 linear meters under BoQ Item 1.3.2. Please refer to Amendment No. 1 issued with this clarification.

	Question No. 2
	Fence Post Foundation Dimensions
BoQ Item 1.3.2 specifies fence post foundations measuring 40 cm × 40 cm × 60 cm, whereas Drawing Sheet A.01.06 indicates dimensions of 50 cm × 50 cm × 100 cm. Please confirm which dimensions shall govern the execution and pricing of the fence post foundations.

	Response
	The governing foundation dimensions shall be 40 cm × 40 cm × 60 cm, as specified in BoQ Item 1.3.2. Please refer to the amended drawing and Amendment No. 1 issued with this clarification.

	Question No. 3
	Structural Steel Purlin Dimensions
Drawing Sheet A.01.05 identifies the module-support purlins and horizontal framework as “4 × 8 mm, 1 mm thick Steel Pipe” and “3 × 6 mm, 1 mm thick Steel Pipe.” Please confirm whether these notations represent 40 mm × 80 mm and 30 mm × 60 mm rectangular steel pipes, respectively.

	Response
	Confirmed. The notations represent 40 mm × 80 mm and 30 mm × 60 mm rectangular steel pipes, respectively. Please refer to the amended drawing and Amendment No. 1 issued with this clarification.

	Question No. 4
	Key Personnel Qualification – Project Manager
Section VII – Works’ Requirements specifies a Bachelor’s Degree in Electrical Engineering for the Project Manager in the Key Staffing and Qualifications table, while the subsequent Key Personnel table specifies a Bachelor’s Degree in Civil Engineering. Please confirm the applicable academic qualification.

	Response
	The Project Manager is required to hold a Bachelor’s Degree in Electrical Engineering and have at least five years of relevant experience in solar projects. Please refer to Amendment No. 1 issued with this clarification.

	Question No. 5
	Pricing of Signboards
Please confirm whether signboards should be priced under BoQ 0 – Preliminaries or exclusively under the dedicated signboard line item included in the respective Lot Financial Offer tables, to avoid duplicate pricing.

	Response
	No signboards are mentioned or required under BoQ 0, Item 1.2. Bidders shall price the required signboards exclusively under the dedicated signboard line item in the respective Lot Financial Offer table. No additional signboard cost shall be included under BoQ 0.
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